neoFootage AI is a powerful pro video processor with AI enhancing designed for quality, speed and ease of use, featuring from fast conversions to complete video transformation and improvement.
Create perfect pro-quality videos with the efficient SDR and HDR workflow with smart batch processing, the intuitive user interface is designed to easily configure the many powerful features with real time preview, just import one, tens, or hundreds of videos, easily configure the processing, and send the videos to the job server to produce professional quality videos in SDR and HDR ready to edit or distribute.
neoFootage AI can handle it all in one simple step and supports all industry standard video formats in NTSC and PAL including SD,HD,4k and 8k,in SDR,HDR and in gamma and color space formats from prosumer and pro cameras.
Features at a glance
Deep learning technology
• Video enhance AI: upsample videos creating details, and restore low quality videos removing compression artifacts like halos, blocking and ringing. 
• SuperChroma AI, upscale and restore video chroma, and remove chroma subsampling artifacts and chroma bleeding.
• SuperBitdepth AI: upscale and restore video bitdepth, remove posterization and banding.
Imports a wide variety of pro and consumer formats and image sequences, captures from HDV firewire cameras
• Pro and consumer codecs with Alpha channel, like DNxHD/DNxHR,AVC-Intra,XAVC,ProRes,XDCAM, Cineform,AVC or HEVC
• Containers like mov, mp4, MXF OP-1a and OP-Atom, avi, mkv, mts, wmv, webm or mpg
Encoding to pro and consumer formats 
• More than 30 pro formats in 8,10,12 bit like DNxHD/DNxHR, ProRes, XDCAM or Cineform and consumer formats like AVC and HEVC
• Pro containers MXF OP1-a and OP-Atom fully compatible with best NLEs
• HDR10 with MaxCLL/MaxFALL calculation and HEVC GPU encoding	
Standards conversions, frame rate conversions, resample
• Conversions with optical flow between all standards and formats,NTSC and PAL,in SD,HD,4K,8K
• Motion adaptive deinterlacing,convert progressive to interlaced, TFF/BFF conversions
• Supports standard, cinema and vertical aspect ratios like 16:9,2.35:1,4:3 DV or 9:16
Advanced color correction with LUT manager and real time preview
• 22 advanced color correction effects
• Apply, preview and create 3DLUTs
• Real time preview in SDR, simulated HDR, and real HDR in Windows HDR display mode
Perfect gamma and color space conversions with advanced tone mapping from more than 100 standard and camera formats
• Supports standard gamma and color spaces like Rec.709,Rec.2020,Rec.601,ST2084/PQ or HLG.
• Support cameras gamma like Panasonic V-log, Sony S-log, Canon log, DJI D-log, GoPro Protune, Fujifilm F-log, Arri LogC and more
• Support cameras color spaces like Sony S-gamut, Panasonic V-gamut, Canon cinema, DJI D-gamut, Fujifilm , Protune and Arri Alexa gamut and more
Convert SDR videos to perfect HDR
• Convert SDR videos from any format,HD,4K,interlaced or progressive to perfect HDR
Convert HDR videos to pristine SDR 
• Convert HDR videos to any SDR video format,SD,HD,4K,interlaced or progressive
Convert from camera gamma and color space formats to perfect SDR and HDR
• Convert directly from your camera to any SDR and HDR video format
Video synchronization with external audio recorders
• Easy and fast sync, no clapping or timecode needed
• Audio drift detection and correction
Powerful job server
• Work on more videos while job server is rendering
Pro features easy to configure
• Smart batch processing
• Trim,split and join videos accurately
• Burn-in filter for timecode or image logo
• Imports timecode from pro formats
• Video denoiser
• Audio conversions and filters
Fast high quality processing
• High quality processing in 32 bit
• Nvidia and Quicksync GPU encoding and decoding
• Multi core CPU with SSE3, AVX and AVX-512 support
• CUDA and OpenCL GPU processing

Find more information and download a free full featured trial version: 
https://www.acrovid.com/neofootage_ai.htm
For any inquiry, please email to:
support@acrovid.com